Specification related to technical drawing zone 2-18

**SPECIFICATIONS** page 1 of 1

 **BALLAST/PERENNIAL ROOF COVER, ROOF GARDEN CARPET**

The build ups specified in the specification and drawing are suitable for roofs with a pitch of

5°-25°.Roofs with a different pitch require a different build-up.

**BALLAST/SEDUM ROOF COVER**

System build-up:

* Water buffering fleece
* Extensive roof garden substrate
* Pre-cultivated vegetation blankets

Total built height 90 mm

Water saturated weight (kg/m2) up to 100 kg/m2 (fully water saturated)

**WATER BUFFERING FLEECE**

* Supplier:
* Type: B1200
* Weight: 1200 g/m2
* Material: Polypropylene, acrylic (available on a roll)
* Thickness (mm): 10 mm
* Standard roll width (m): 2,00
* Install on drainage

**SUBSTRATE**

* Supplier:
* Type: extensive roof garden substrate
* Material: based on FLL guidelines
* Layer thickness after subsidence (mm): 50 mm
* Characteristic feature: excellent drainage

**VEGETATION/PLANTS**

* Supplier: Sempergreen® (+31 343 539699)
* Type: Sempergreen® pre-cultivated Sedum vegetation blanket cultivated on biodegradable coconut fibre
* Cultivated on a Sempergreen® cultivation substrate
* Coverage upon delivery / installation: 95%
* Plant mixture: 10 to 12 different kinds of Sedum
* Standard roll width (m): 1,00/1,20. Available in other widths upon request
* Standard roll length (m): 1,00/2,00. Available in other lengths upon request
* Delivery: on roll/on pallet
* Saturate the build-up with water after the vegetation blankets have been installed

**ACCESSORIES**

* Supplier:
* Gravel (optional)
* Roof edge profile (optional)
* Separator (optional)
* Inspection pit (optional)
* Bulb wire grille (optional)
* Leaf trap (optional)
* Tile support (optional)

**PROCESS**

Processing based on FLL guidelines and in accordance with the supplier's guidelines and instructions.